---- task[T:\\hci\_test\\TPCFCBV-02-C.lua]begin ----

usb id [0xffff] ok

usb id [0xffff] ok

CMD hci\_le\_read\_buf\_size

<-------------------------------------------------------------------------------------

01 02 20 00

HCI\_Command\_Complete\_Event

-------------------------------------------------------------------------------------->

Status: 0x00

HC\_LE\_Data\_Packet\_Length: 0x001b

HC\_Total\_Num\_LE\_Data\_Packets: 0x02x

CMD hci\_read\_buffer\_size

<-------------------------------------------------------------------------------------

01 05 10 00

HCI\_Command\_Complete\_Event

-------------------------------------------------------------------------------------->

Status: 0x00

04 0e 0b 01 05 10 00

HC\_ACL\_Data\_Packet\_Length: 0x0136

HC\_Synchronous\_Data\_Packet\_Length: 0x02x

HC\_Total\_Num\_ACL\_Data\_Packets: 0x000a

HC\_Total\_Num\_Synchronous\_Data\_Packets: 0x0008