---- task[T:\\hci\_test\\TPCINBV-06-C.lua]begin ----

usb id [0xffff] ok

usb id [0xffff] ok

CMD hci\_le\_clear\_white\_list

<-------------------------------------------------------------------------------------

01 10 20 00

HCI\_Command\_Complete\_Event

-------------------------------------------------------------------------------------->

Status: 0x00

CMD hci\_le\_read\_white\_list\_size

<-------------------------------------------------------------------------------------

01 0f 20 00

HCI\_Command\_Complete\_Event

-------------------------------------------------------------------------------------->

Status: 0x00

White\_List\_Size: 0x04

Repeat 4 times to send HCI CMD: hci\_le\_add\_dev\_2\_white\_list

CMD hci\_le\_add\_dev\_2\_white\_list

<-------------------------------------------------------------------------------------

01 11 20 07 00 11 34 12 ef cd ab

addr\_type:00, addr:0xabcdef123411

HCI\_Command\_Complete\_Event

-------------------------------------------------------------------------------------->

Status: 0x00

CMD hci\_le\_add\_dev\_2\_white\_list

<-------------------------------------------------------------------------------------

01 11 20 07 00 22 34 12 ef cd ab

addr\_type:00, addr:0xabcdef123422

HCI\_Command\_Complete\_Event

-------------------------------------------------------------------------------------->

Status: 0x00

CMD hci\_le\_add\_dev\_2\_white\_list

<-------------------------------------------------------------------------------------

01 11 20 07 00 33 34 12 ef cd ab

addr\_type:00, addr:0xabcdef123433

HCI\_Command\_Complete\_Event

-------------------------------------------------------------------------------------->

Status: 0x00

CMD hci\_le\_add\_dev\_2\_white\_list

<-------------------------------------------------------------------------------------

01 11 20 07 00 44 34 12 ef cd ab

addr\_type:00, addr:0xabcdef123444

HCI\_Command\_Complete\_Event

-------------------------------------------------------------------------------------->

Status: 0x00

CMD hci\_le\_add\_dev\_2\_white\_list

<-------------------------------------------------------------------------------------

01 11 20 07 00 aa 34 12 ef cd ab

addr\_type:00, addr:0xabcdef1234aa

HCI\_Command\_Complete\_Event

-------------------------------------------------------------------------------------->

Status: 0x41

CMD le\_remove\_device\_to\_whitelist

<-------------------------------------------------------------------------------------

01 12 20 07 00 11 34 12 ef cd ab

addr\_type:00, addr:0xabcdef123411

HCI\_Command\_Complete\_Event

-------------------------------------------------------------------------------------->

Status: 0x00

CMD hci\_le\_add\_dev\_2\_white\_list

<-------------------------------------------------------------------------------------

01 11 20 07 00 aa 34 12 ef cd ab

addr\_type:00, addr:0xabcdef1234aa

HCI\_Command\_Complete\_Event

-------------------------------------------------------------------------------------->

Status: 0x00

end!