---- task[T:\\hci\_test\\TPDSUBV-02-C.lua]begin ----

usb id [0xffff] ok

usb id [0xffff] ok

HCI\_LE\_Set\_Advertising\_Parameters

<-------------------------------------------------------------------------------------

01 06 20 0f 20 00 20 00 00 00 00 1c fb 62 38 c1 a4 01 00

intervalMin: 0020

intervalMax: 0020

advType: 00

ownAddrType: 00

peerAddrType: 00

peerAddr: 0xa4c13862fb1c

adv\_channelMap: 01

advFilterPolicy: 00

HCI\_Command\_Complete\_Event

-------------------------------------------------------------------------------------->

Status: 0x00

HCI\_LE\_Set\_Advertise\_Enable

<-------------------------------------------------------------------------------------

01 0a 20 01 01

(Enable)

HCI\_Command\_Complete\_Event

-------------------------------------------------------------------------------------->

Status: 0x00

CMD hci\_reset

<-------------------------------------------------------------------------------------

01 03 0c 00

HCI\_Command\_Complete\_Event

-------------------------------------------------------------------------------------->

Status: 0x00

end!