---- task[T:\\hci\_test\\TPDSUBV-05-C.lua]begin ----

usb id [0xffff] ok

usb id [0xffff] ok

CMD hci\_le\_create\_conn

<-------------------------------------------------------------------------------------

01 0d 20 19 a0 00 a0 00 00 00 1c fb 62 38 c1 a4 00 18 00 18 00 00 00 90 01 00 00 00 00

LE\_Scan\_Interval: 00a0

LE\_Scan\_Window: 00a0

Initiator\_Filter\_Policy: 00

Peer\_Address\_Type: 00

Peer\_Address: 0xa4c13862fb1c

Own\_Address\_Type: 00

Conn\_Interval\_Min: 0018

Conn\_Interval\_Max: 0018

Conn\_Latency: 0000

Supervision\_Timeout: 0190

Minimum\_CE\_Length: 0000

Maximum\_CE\_Length 0000

HCI\_Command\_Status\_Event

-------------------------------------------------------------------------------------->

Status: 0x00

TEST OK!

CMD hci\_reset

<-------------------------------------------------------------------------------------

01 03 0c 00

HCI\_Command\_Complete\_Event

-------------------------------------------------------------------------------------->

Status: 0x00

end!