---- task[T:\\hci\_test\\TPHFCBV-04-C.lua]begin ----

usb id [0xffff] ok

usb id [0xffff] ok

hci\_cmd\_le\_set\_event\_mask

<-------------------------------------------------------------------------------------

01 01 20 08 89 18 00 00 00 80 00 20

EventMask: 0x2000800000001889

HCI\_Command\_Complete\_Event

-------------------------------------------------------------------------------------->

Status: 0x00

04 0e 04 01 01 20 00

hci\_cmd\_le\_set\_event\_mask

<-------------------------------------------------------------------------------------

01 01 20 08 1d 00 00 00 00 00 00 00

EventMask: 0x000000000000001d

HCI\_Command\_Complete\_Event

-------------------------------------------------------------------------------------->

Status: 0x00

04 0e 04 01 01 20 00

HCI\_LE\_Set\_Scan\_Parameters

<-------------------------------------------------------------------------------------

01 0b 20 07 01 10 02 10 02 00 00

Active Scanning, Policy: 0x00

Scan\_interval: 0220

Scan\_window: 0220

OwnAddrType: 00

Filter\_policy: 00

HCI\_Command\_Complete\_Event

-------------------------------------------------------------------------------------->

Status: 0x00

CMD HCI\_LE\_Set\_SCAN\_Enable

<-------------------------------------------------------------------------------------

01 0c 20 01 01

(Enable)

HCI\_Command\_Complete\_Event

-------------------------------------------------------------------------------------->

Status: 0x00

CMD HCI\_LE\_Set\_SCAN\_Enable

<-------------------------------------------------------------------------------------

01 0c 20 01 00

(Disable)

HCI\_Command\_Complete\_Event

-------------------------------------------------------------------------------------->

Status: 0x00

CMD hci\_le\_create\_conn

<-------------------------------------------------------------------------------------

01 0d 20 19 a0 00 a0 00 00 00 1c fb 62 38 c1 a4 00 18 00 18 00 00 00 90 01 00 00 00 00

LE\_Scan\_Interval: 00a0

LE\_Scan\_Window: 00a0

Initiator\_Filter\_Policy: 00

Peer\_Address\_Type: 00

Peer\_Address: 0xa4c13862fb1c

Own\_Address\_Type: 00

Conn\_Interval\_Min: 0018

Conn\_Interval\_Max: 0018

Conn\_Latency: 0000

Supervision\_Timeout: 0190

Minimum\_CE\_Length: 0000

Maximum\_CE\_Length 0000

HCI\_Command\_Status\_Event

-------------------------------------------------------------------------------------->

Status: 0x00

HCI\_LE\_Connection\_Complete\_Event

===========================================>

Status: 0x00

connection\_handle: 0080

role 0x00

Peer\_Address\_Type 00

peerAddr: 0xa4c13862fb1c

Conn\_Interval: 0x0010

Conn\_Latency: 0x0000

Supervision\_Timeout: 0x0190

Master\_Clock\_Accuracy: 00

end!