---- task[T:\\hci\_test\\TPCINBV-04-C.lua]begin ----

usb id [0xffff] ok

usb id [0xffff] ok

CMD hci\_read\_local\_ver\_info

<-------------------------------------------------------------------------------------

01 01 10 00

HCI\_Command\_Complete\_Event

-------------------------------------------------------------------------------------->

Status: 0x00

HCI\_Version: 0x06

HCI\_Revision: 0x22bb

LMP/PAL\_Version: 0x06

Manufacturer\_Name: 0x0211

LMP/PAL\_Subversion: 0xbb02